# .font: font.text_2
# .autowrap: false
# .centered: true
AM24 02A Creedite
# .font: font.text_1
by
# .font: font.text_2
altermaven
# .centered: false

# .font: font.value_1
# .autowrap: false
ALTERMAVEN                        2024-03-09 22:23
# .font: font.value_2
# .autowrap: true
TRYING TO GENERATE A GOOD RUN-THROUGH CAVE IS A BIT DIFFICULT, AND THEY REALLY DON'T HAVE ANY GIMMICKS ASIDE FROM DEXTERITY TESTING. REGARDLESS, THIS WAS ONE PARTICULAR LAYOUT THAT DIDN'T SIT WITH ME..  
  
CREEDITE IS ACTUALLY A HALIDE MATERIAL, AND VIOLET CREEDITE IS ONE OF THE VARIANTS WITNESSED. IN THIS CASE, IT IS A HEAVILY OXIDIZED VARIANT OF FLUORITE.  
  
IT HAS A MOHS HARDNESS OF 4.